|  |
| --- |
| **PLUMBING / FUEL GAS****TAC ACTION/Votes****Local Technical amendments****to the****2020 7th Edition Florida Building Code** |
|  |  |  |  |
| **JURISDICTION** | **DOCUMENT with TECHNICAL AMENDMENT** | **SUMMARY OF TECHNICAL AMENDMENT** | **TAC ACTION/VOTE** |
|  |  |  |  |
| Pinellas CountyConstruction Industry Licensing Board(PCCLB) | FBC –Residential P2906.9.1.4 P2903.2.1P2903.1P2705.1FBC- Plumbing Sec 705.10.2Sec. 610.2Sec 605.21.3 | AMEND EXISTING SECTION**Section P2906.9.1.4 PVC plastic pipe**. A purple primer that conforms to ASTM F656 shall be applied to PVC solvent-cemented joints. Solvent cement for PVC plastic pipe conforming to ASTM D 2564 shall be applied to all joint surfaces.Exception: Clear Primer conforming to ASTM F656 may be used on any exposed PVC pipe or fittings on trim/finish work.**Section P2903.2.1** – amendment to add provisions pertaining to minimum water service size.**Section P2903.1** – amendment to clarify that disinfection is not required every time work is performed on a plumbing system.**Section P2705.1** – amendment to bring awareness to the plumbing fixture spacing requirements located in both sections of the code.**Section 705.10.2** – amendment to permit the use of clear primer instead of purple primer when used on exposed PVC pipe or fittings on trim/finish work.**Section 610.2** - amendment to clarify that disinfection is not required every time work is performed on a plumbing system.**Section 65.21.3** – amendment to permit the use of clear primer instead of purple primer when used on exposed PVC pipe or fittings or trim/finish work. | VOTE: |
|  |  |  |  |
| County of Palm Beach | FBC – PlumbingAppendix F | Amendment to adopt Appendix F “Proposed Construction Building Codes for Turf and Landscape Irrigation System” | VOTE: |
|  |  |  |  |
| County of Miami-Dade | FBC – PlumbingSec 604.4Table 604.4FBC - ResidentialP2903.2 and Table P2903.2 | Sections 604.4/P2903.2 – amendments to meet the water conservation goals provided in the County’s Water Efficiency Plan. | Vote: |
|  |  |  |  |
| County of Broward | FBC – Residential Table P2903.2 | Table P2903.2 – amendment revising the maximum flow rates and consumption for plumbing fixture, fixture fittings and appliances. | VOTE: |
|  |  |  |  |
| County of Broward | FBC – PlumingSec 314.2.1 | Section 314.2.1 – amendment to require the collection of condensate from all cooling coils and evaporators of equipment serviced by on- site cooling tower in a building or structure wherein the aggregate cooling capacity of the equipment exceeds 65,000 BTU/HR. | VOTE: |
|  |  |  |  |
| County of Miami-Dade | FBC – PlumbingSec 604.4 | Section 604.4 – amendment reducing plumbing fixture water flow rates currently required by the FBC – Plumbing thereby increasing water conservation standards.  |  |
|  |  |  |  |
|  |  |  |  |
| County of Broward | FBC – PlumbingAppendix F | Amendment to adopt Appendix F “Proposed Construction Building Codes for Turf and Landscape Irrigation System” | VOTE: |
|  |  |  |  |
| County of Broward | FBC – PlumbingSec 307.2.1 | Section 307.2.1- amendment to require the collection of condensate from all cooling coils and evaporators of equipment serviced by on- site cooling tower in a building or structure wherein the aggregate cooling capacity of the equipment exceeds 65,000 BTU/HR. | VOTE: |
|  |  |  |  |

|  |
| --- |
| **FUEL GAS****TAC Action Votes to the****Local Technical Amendments** **2020 7th Building Code** |
|  |  |  |  |
| **JURISDICTION** | **DOCUMENT with****TECHNICAL****AMENDMENT** | **TEXT OF TECHNICAL AMENDMENT** | **TAC REVIEW** |
|  |  |  |  |
| Pinellas County Construction Industry Licensing Board(PCCLB) | FBC – Residential G2415.15FBC – Fuel Gas Sec 404.15 | Section G2415.15 - amendment to add limitations to control future connections to gas outlets.Section 404.15 – amendment to add limitations to control future connections to gas outlets.  | VOTE: |
|  |  |  |  |