**From:** Whitehead, Don [mailto:Don.Whitehead@fldoe.org]
**Sent:** Monday, July 26, 2021 8:50 AM
**To:** Madani, Mo
**Subject:** RE: Errata Submittal Time line – July 1, 2021 to July 14-2021

|  |
| --- |
| **[NOTICE] This message comes from a system outside of DBPR. Please exercise caution when clicking on links and/or providing sensitive information. If you have concerns, please contact your Knowledge Champion or the DBPR Helpdesk.** |

Mo,

This error was just brought to our attention, that ASCE 7 changed their figure numbering from Figure 26.5-1B in ASCE 7-10 to Figure 26.5-1C in ASCE 7-16. Is it possible to add this to the change that we have already submitted or is there some other way to add this change to the errata?

**453.9.1 Loading requirements.** Structural design shall

comply with code requirements and wind loads as stipulated

by the *Florida Building Code* and the *Florida Fire*

*Prevention Code* as adopted by the State Fire Marshal.

Wind design shall be based on ASCE 7, with wind speeds

determined from Figure 26.5-1~~B~~C and ICC 500, as appropriate.

Don S. Whitehead, AIA, LEED AP

Safe and Efficient Facilities Design Manager

Office of Educational Facilities

Florida Department of Education

(850) 245-9295